All Spencer Walcott [Hancock Classics] window units come standard with ¾” Clear Insulating Glass.

The following glazing options are also available:

Insulating Low-e

Insulating Low-e with Argon gas fill

PassivGlas (8070) Low-e with Argon gas fill

Insulating Laminated Safety

Insulating Obscure

Insulating Low-e/Obscure

Insulating Low-e/Obscure with Argon gas fill

Insulating Clear Tempered

Insulating Low-e Tempered with Argon gas fill

Insulating Obscure Tempered

Insulating Low-e/Obscure Tempered with Argon gas fill